{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["废水"],"not_rendered":{"external_links":2,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"废水","index":0,"n_rows":7,"n_cols":9,"rows_kept":7,"merged":[[0,0,0,8],[5,0,5,8]],"flags":["formulas_cached_only"]}
["广州市2018年国控企业污染源（废水重点）监督性监测结果（第三季度9月）"]
["行政区","企业名称","监测点名称","执行标准名称","监测日期","监测项目名称（单位）","污染物浓度","标准限值","是否达标"]
["南沙区","广州市宏杰达纸业有限公司","污水站处理后","化学需氧量、氨氮两项执行《制浆造纸工业水污染物排放标准》（GB3544-2008)的表3水污染物特别排放限值（制浆和造纸联合生产企业），其它指标执行表2标准","2018-08-23","可吸附有机卤素（mg/L）",0.082,12,"是"]
["南沙区"," 广州造纸股份有限公司","总排放口","化学需氧量、氨氮两项执行《制浆造纸工业水污染物排放标准》（GB3544-2008)的表3水污染物特别排放限值（制浆和造纸联合生产企业），其它指标执行表2标准","2018-08-23","可吸附有机卤素（mg/L）",0.11,12,"是"]
["增城区","广州市穗新牧业有限公司","总排放口","《水污染物排放限值》（DB44/26-2001）第二时段一级标准+《禽畜养殖业污染排放标准》（DB44/613-2009）表5集约化畜禽养殖业污染最高允许日均排放浓度（珠三角标准值）","2018-08-23","蛔虫卵（个/10L）","ND","/","/"]
["备注： ①结果中“ND”表示未检出，蛔虫卵检出限为20MPN/L。"]
[null,"② 可吸附有机卤素、蛔虫卵项目是属于分包数据，由中国广州分析测试中心提供。"]